Assembly Manual Template
Free template from Manual to Video (manualtovideo.com). Replace everything in [brackets]. Free to use and change.
1. Cover and product ID
Product name: [name]
Model / article number: [number]
Version and date of this manual: [v1.0, month year]
[Picture of the finished product]
Manufacturer: [company name, postal address, website, email]
In the EU, the manufacturer's name and contact address must be on the product, its packaging or a document that comes with it.
2. Safety first
[Most serious warning first, e.g. Tip-over risk: always fix this product to the wall with the wall anchor supplied.]
[e.g. Small parts: keep away from children under 3 during assembly.]
[e.g. Two people needed for steps 5 to 7.]
Read all steps before you start. Keep this manual.
3. Before you start
Time needed: [about 45 minutes]
People needed: [1 / 2]
Tools needed: [cross-head screwdriver, Allen key (supplied), hammer]
Work area: lay the parts on a soft, clean surface, such as the box opened flat.
Check the parts and hardware against the lists below before you start.
4. Parts
	Letter
	Part
	Qty
	Picture

	A
	[Side panel]
	[2]
	[drawing]

	B
	[Top panel]
	[1]
	[drawing]

	C
	[Shelf]
	[3]
	[drawing]

	D
	[Back panel]
	[1]
	[drawing]



5. Hardware
	No.
	Item
	Qty
	Actual size

	1
	[Screw M6 x 30]
	[8]
	[drawing at 1:1]

	2
	[Wooden dowel 8 x 30]
	[12]
	[drawing at 1:1]

	3
	[Cam lock]
	[8]
	[drawing at 1:1]

	4
	[Wall anchor kit]
	[1]
	[drawing at 1:1]



6. Steps
	Step
	Action
	Parts and hardware
	Picture
	Tip or warning

	1
	[One action only, e.g. Push dowels (2) into the side panel (A).]
	[A x1, 2 x6]
	[drawing: arrows show direction]
	[e.g. Do not glue yet.]

	2
	[e.g. Fit the shelves (C) between the side panels.]
	[C x3]
	[drawing]
	[e.g. The holes face down.]

	3
	[e.g. Turn the cam locks (3) a half turn clockwise.]
	[3 x8]
	[drawing, close-up of the lock]
	



7. Final check
[ ] Every screw is tight.
[ ] The product stands level and does not rock.
[ ] It is fixed to the wall (see safety).
[ ] No parts or hardware are left over.
8. Care and maintenance
[e.g. Check and tighten the screws every 6 months.]
[e.g. Clean with a dry cloth.]
9. Help
Watch these steps as a video: [QR code + link]. Make a free QR code at manualtovideo.com/tools/qr-code.
Missing or damaged parts: [phone, email, website]. Have your model number ready: [number].
Turn this manual into an animated assembly video: manualtovideo.com
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